|  |  |  |
| --- | --- | --- |
| Pre-Project (Existing) Land Cover | Post-Project Land Cover | Flow Control Requirements  |
| Forested | New Impervious | Project Site: Provide onsite flow control BMPs to match predeveloped (forested) conditions.Flow Control Improvement Transfer: Not Allowed |
| Lawn/Landscaped | New Impervious | Project Site: Provide onsite flow control BMPs to match pre-project (lawn/landscaped) conditions.Flow Control Improvement Transfer: Transfer flow control improvements to match pre-project (lawn/landscaped) flow durations to predeveloped (forested) flow durations.  |

|  |
| --- |
|  |
| Pre-Project (Existing) Land Cover | Post-~~Developed~~ Project Land Cover | Flow Control Requirement(s) ~~to be added as part of the Development Project~~ |
| 0.5 acres Forested | 0.5 acres New Impervious | Project Site: Provide onsite flow control BMPs to match post-project (0.5 acres impervious) to pre-project (0.5 Acres Forested) ~~Impervious to Forested~~ conditions.~~Transfer Site~~ Flow Control Improvement Transfer: ~~No Additional Improvements (transfer not allowed)~~ Not Allowed. |
| 3.3 acres Pasture | 3.3 acres New Impervious | Project Site: Provide onsite flow control BMPs to match post-project (3.3 acres impervious) to pre-project (3.3 acres pasture) conditions. ~~Acres Impervious to Forested~~Flow Control Improvement Transfer ~~Site~~: Transfer flow control improvements to match pre-project (3.3 acres pasture) flow durations to predeveloped (3.3 acres forested) flow durations. ~~3.3 Acres Pasture to Forest~~ |
| 1.0 acre Lawn/Landscape | 1.0 acre New Impervious | Project site: Provide onsite flow control BMPs to match post-project (1.0 acres impervious) to pre-project (1.0 acres lawn/landscape) conditions. ~~1.0 acre Impervious to lawn/landscape~~Flow Control Improvement Transfer ~~site~~: Transfer flow control improvements to match pre-project (1.0 acre lawn/landscape) flow durations to predeveloped (1.0 acres forested) flow durations. ~~1.0 acre lawn/landscape to forested~~ |
| 0.2 Effective Impervious | 0.2 Replaced Impervious | Project site: ~~No Additional Improvements~~ Not Allowed.Flow Control Improvement Transfer ~~site~~: Transfer flow control improvements to match pre-project (0.2 acre impervious) flow durations to predeveloped (0.2 acres forested) flow durations. ~~0.2 acre Impervious to forested~~ |